# Copyright:	Public domain.
# Filename:	WAITLIST.agc
# Purpose:	Part of the source code for Colossus 2A, AKA Comanche 055.
#		It is part of the source code for the Command Module's (CM)
#		Apollo Guidance Computer (AGC), for Apollo 11.
# Assembler:	yaYUL
# Contact:	Ron Burkey <info@sandroid.org>.
# Website:	www.ibiblio.org/apollo.
# Pages:	1221-1235
# Mod history:	2009-05-14 RSB	Adapted from the Colossus249/ file of the
#				same name, using Comanche055 page images.
#
# This source code has been transcribed or otherwise adapted from digitized
# images of a hardcopy from the MIT Museum.  The digitization was performed
# by Paul Fjeld, and arranged for by Deborah Douglas of the Museum.  Many
# thanks to both.  The images (with suitable reduction in storage size and
# consequent reduction in image quality as well) are available online at
# www.ibiblio.org/apollo.  If for some reason you find that the images are
# illegible, contact me at info@sandroid.org about getting access to the
# (much) higher-quality images which Paul actually created.
#
# Notations on the hardcopy document read, in part:
#
#	Assemble revision 055 of AGC program Comanche by NASA
#	2021113-051.  10:28 APR. 1, 1969
#
#	This AGC program shall also be referred to as
#			Colossus 2A

# Page 1221
# PROGRAM DESCRIPTION						DATE - 10 OCTOBER 1966
# MOD NO - 2							LOG SECTION - WAITLIST
# MOD BY - MILLER	(DTMAX INCREASED TO 162.5 SEC)		ASSEMBLY SUNBURST REV 5
# MOD 3 BY KERNAN	(INHINT INSERTED AT WAITLIST) 2/28/68 SKIPPER REV 4
# MOD 4BY KERNAN	(TWIDDLE IN 54) 3/28/68 SKIPPER REV 13.
#
# FUNCTIONAL DESCRIPTION-
#	PART OF A SECTION OF PROGRAMS,-WAITLIST, TASKOVER, T3RUPT, USED TO CALL A PROGRAM, (CALLED A TASK),
#	WHICH IS TO BEGIN IN C(A) CENTISECONDS.  WAITLIST UPDATES TIME3, LST1 AND LST2. THE MEANING OF THESE LISTS
#	FOLLOW.
#
#		C(TIME3) = 16384 -(T1-T) CENTISECONDS, (T=PRESENT TIME, T1-TIME FOR TASK1)
#
#			C(LST1)		=	-(T2-T1)+1
#			C(LST1 +1)	=	-(T3-T2)+1
#			C(LST1 +2)	=	-(T4-T3)+1
#				       ...
#			C(LST1 +6)	=	-(T8-T7)+1
#			C(LST1 +7)	=	-(T9-T8)+1
#
#			C(LST2)		=	2CADR OF TASK1
#			C(LST2 +2)	=	2CADR OF TASK2
#				       ...
#			C(LST2 +14)	=	2CADR OF TASK8
#			C(LST2 +16)	=	2CADR OF TASK9
#
# WARNINGS-
# --------
#	1)	1 <= C(A) <= 16250D (1 CENTISECOND TO 162.5 SEC)
#	2)	9 TASKS MAXIMUM
#	3)	TASKS CALLED UNDER INTERRUPT INHIBITED
#	4)	TASKS END BY TC TASKOVER
#
# CALLING SEQUENCE-
#
#	L-1	CA	DELTAT 	(TIME IN CENTISECONDS TO TASK START)
#	L	TC	WAITLIST
#	L+1	2CADR	DESIRED TASK
#	L+2	(MINOR OF 2CADR)
#	L+3	RELINT		(RETURNS HERE)
#
# TWIDDLE-
# -------
#	TWIDDLE IS FOR USE WHEN THE TASK BEING SET UP IS IN THE SAME EBANK AND FBANK AS THE USER.  IN
#	SUCH CASES, IT IMPROVES UPON WAITLIST BY ELIMINATING THE NEED FOR THE BBCON HALF OF THE 2CADR,
# Page 1222
#	SAVING A WORD.  TWIDDLE IS LIKE WAITLIST IN EVERY RESPECT EXCEPT CALLING SEQUENCE, TO WIT-
#
#		L-1	CA	DELTAT
#		L	TC	TWIDDLE
#		L+1	ADRES	DESIRED TASK
#		L+2	RELINT		(RETURNS HERE)
#
# NORMAL EXIT MODES-
#
#	AT L+3 OF CALLING SEQUENCE
#
# ALARM OR ABORT EXIT MODES-
#
#	TC	ABORT
#	OCT	1203	(WAITLIST OVERFLOW - TOO MANY TASKS)
#
# ERASABLE INITIALIZATION REQUIRED-
#
#	ACCOMPLISHED BY FRESH START,--	LST2,..., LST2 +16 =ENDTASK
#					LST1,..., LST1 +7  =NEG1/2
#
# OUTPUT--
#
#	LST1 AND LST2 UPDATED WITH NEW TASK AND ASSOCIATED TIME.
# DEBRIS-
#	CENTRALS- A,Q,L
#	OTHER   - WAITEXIT, WAITADR, WAITTEMP, WAITBANK
# DETAILED ANALYSIS OF TIMING-
#
#	CONTROL WILL NOT BE RETURNED TO THE SPECIFIED ADDRESS (2CADR) IN EXACTLY DELTA T CENTISECONDS.
#	THE APPROXIMATE TIME MAY BE CALCULATED AS FOLLOWS
#
#		LET T0 = THE TIME OF THE TC WAITLIST
#		LET TS = T0 +147U + COUNTER INCREMENTS (SET UP TIME)
#		LET X  = TS -(100TS)/100  (VARIANCE FROM COUNTERS)
#		LET Y  = LENGTH OF TIME OF INHIBIT INTERRUPT AFTER T3RUPT
#		LET Z  = LENGTH OF TIME TO PROCESS TASKS WHICH ARE DUE THIS T3RUPT BUT DISPATCHED EARLIER.
#	(Z=0, USUALLY)
#		LET DELTD = THE ACTUAL TIME TAKEN TO GIVE CONTROL TO 2CADR
#	       THEN DELTD = TS+DELTA T -X +Y +Z +1.05MS* +COUNTERS*
#	*THE TIME TAKEN BY WAITLIST ITSELF AND THE COUNTER TICKING DURING THIS WAITLIST TIME.
#
#	IN SHORT, THE ACTUAL TIME TO RETURN CONTROL TO A 2CADR IS AUGMENTED BY THE TIME TO SET UP THE TASK'S
# 	INTERRUPT, ALL COUNTERS TICKING, THE T3RUPT PROCESSING TIME, THE WAITLIST PROCESSING TIME AND THE POSSIBILITY
#	OF OTHER TASKS INHIBITING THE INTERRUPT.

		BLOCK	02
# Page 1223
		EBANK=	LST1		# TASK LISTS IN SWITCHED E BANK.

		COUNT	02/WAIT

TWIDDLE		INHINT
		TS	L		# SAVE DELAY TIME IN L
		CA	POSMAX
		ADS	Q		# CREATING OVERFLOW AND Q-1 IN Q
		CA	BBANK
		EXTEND
		ROR	SUPERBNK
		XCH	L

WAITLIST	INHINT
		EXTEND
		BZMF	WATLST0-
		XCH	Q		# SAVE DELTA T IN Q AND RETURN IN
		TS	WAITEXIT	# WAITEXIT.
		EXTEND
		INDEX	WAITEXIT	# IF TWIDDLING, THE TS SKIPS TO HERE
		DCA	0		# PICK UP 2CADR OF TASK.
	-1	TS	WAITADR		# BBCON WILL REMAIN IN L
DLY2		CAF	WAITBB		# ENTRY FROM FIXDELAY AND VARDELAY.
		XCH	BBANK
		TCF	WAIT2

WATLST0-	TC	POODOO
		OCT	1204		# WAITLIST CALL WITH ZERO OR NEG DT

# RETURN TO CALLER AFTER TASK INSERTION:

LVWTLIST	DXCH	WAITEXIT
		AD	TWO
		DTCB

		EBANK=	LST1
WAITBB		BBCON	WAIT2

# RETURN TO CALLER +2 AFTER WAITING DT SPECIFIED AT CALLER +1.

FIXDELAY	INDEX	Q		# BOTH ROUTINES MUST BE CALLED UNDER
		CAF	0		# WAITLIST CONTROL AND TERMINATE THE TASK
		INCR	Q		# IN WHICH THEY WERE CALLED.

# RETURN TO CALLER +1 AFTER WAITING THE DT AS ARRIVING IN A.

VARDELAY	XCH	Q		# DT TO Q.  TASK ADRES TO WAITADR.
		TS	WAITADR
		CA	BBANK		# BBANK IS SAVED DURING DELAY.
		EXTEND
# Page 1224
		ROR	SUPERBNK	# ADD SBANK TO BBCON.
		TS	L
		CAF	DELAYEX
		TS	WAITEXIT	# GO TO TASKOVER AFTER TASK ENTRY.
		TCF	DLY2

DELAYEX		TCF	TASKOVER -2	# RETURNS TO TASKOVER

# Page 1225
# ENDTASK MUST ENTERED IN FIXED-FIXED SO IT IS DISTINGUISHABLE BY ITS ADRES ALONE.

		EBANK=	LST1
ENDTASK		-2CADR	SVCT3


SVCT3		CCS	FLAGWRD2	# DRIFT FLAG
		TCF	TASKOVER
		TCF	TASKOVER
		TCF	+1

		CCS	IMUCADR		# DON'T DO NBDONLY IF SOMEONE ELSE IS IN
		TCF	SVCT3X
		TCF	+3
		TCF	SVCT3X
		TCF	SVCT3X
	+3	CAF	PRIO35		# COMPENSATE FOR NBD COEFFICIENTS ONLY.
		TC	NOVAC		#	ENABLE EVERY 81.93 SECONDS
		EBANK=	NBDX
		2CADR	NBDONLY

		TCF	TASKOVER

		SETLOC	FFTAG6
		BANK

SVCT3X		TC	FIXDELAY	# DELAY MAX OF 2 TIMES FOR IMU ZERO
		DEC	500
		TC	SVCT3		# CHECK DRIFT FLAG AGAIN

# Page 1226
# BEGIN TASK INSERTION.

		BANK	01
		COUNT	01/WAIT

WAIT2		TS	WAITBANK	# BBANK OF CALLING PROGRAM.
		CS	TIME3
		AD	BIT8		# BIT 8 = OCT 200
		CCS	A		# TEST 200 - C(TIME3).  IF POSITIVE,
					# IT MEANS THAT TIME3 OVERFLOW HAS OCCURRED PRIOR TO CS TIME3 AND THAT
					# C(TIME3) = T - T1, INSTEAD OF 1.0 - (T1 - T).  THE FOLLOWING FOUR
					# ORDERS SET C(A) = TD - T1 + 1 IN EITHER CASE.

		AD	OCT40001	# OVERFLOW HAS OCCURRED.  SET C(A) =
		CS	A		# T - T1 + 1.0 - 201

# NORMAL CASE (C(A) NNZ) YIELDS SAME C(A):  -( -(1.0-(T1-T)) + 200) - 1

		AD	OCT40201
		AD	Q		# RESULT = TD - T1 + 1.

		CCS	A		# TEST TD - T1 + 1

		AD	LST1		# IF TD - T1 POS, GO TO WTLST5 WITH
		TCF	WTLST5		# C(A) = (TD - T1) + C(LST1) = TD-T2+1

		NOOP
		CS	Q

# NOTE THAT THIS PROGRAM SECTION IS NEVER ENTERED WHEN T-T1 G/E -1,
# SINCE TD-T1+1 = (TD-T) + (T-T1+1), AND DELTA T = TD-T G/E +1.  (G/E
# SYMBOL MEANS GREATER THAN OR EQUAL TO).  THUS THERE NEED BE NO CON-
# CERN OVER A PREVIOUS OR IMMINENT OVERFLOW OF TIME3 HERE.

		AD	POS1/2		# WHEN TD IS NEXT, FORM QUANTITY
		AD	POS1/2		#	1.0 - DELTA T = 1.0 - (TD - T)
		XCH	TIME3
		AD	NEGMAX
		AD	Q		# 1.0 - DELTAT T NOW COMPLETE.
		EXTEND			# ZERO INDEX Q.
		QXCH	7		# (ZQ)

# Page 1227
WTLST4		XCH	LST1
		XCH	LST1 	+1
		XCH	LST1 	+2
		XCH	LST1 	+3
		XCH	LST1 	+4
		XCH	LST1 	+5
		XCH	LST1 	+6
		XCH	LST1 	+7

		CA	WAITADR		# (MINOR PART OF TASK CADR HAS BEEN IN L.)
		INDEX	Q
		TCF	+1

		DXCH	LST2
		DXCH	LST2 	+2
		DXCH	LST2 	+4
		DXCH	LST2 	+6
		DXCH	LST2 	+8D
		DXCH	LST2 	+10D	# AT END, CHECK THAT C(LST2 +10) IS STD
		DXCH	LST2 	+12D
		DXCH	LST2 	+14D
		DXCH	LST2 	+16D
		AD	ENDTASK		# END ITEM, AS CHECK FOR EXCEEDING
					# THE LENGTH OF THE LIST.
		EXTEND			# DUMMY TASK ADRES SHOULD BE IN FIXED-
		BZF	LVWTLIST	# FIXED SO ITS ADRES ALONE DISTINGUISHES
		TCF	WTABORT		# IT.

# Page 1228
WTLST5		CCS	A		# TEST TD - T2 + 1
		AD	LST1 +1
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	1

	+4	CCS	A		# TEST TD - T3 + 1
		AD	LST1 +2
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	2

	+4	CCS	A		# TEST TD - T4 + 1
		AD	LST1 +3
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	3

	+4	CCS	A		# TEST TD - T5 + 1
		AD	LST1 +4
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	4

	+4	CCS	A		# TEST TD - T6 + 1
		AD	LST1 +5
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	5

	+4	CCS	A		# TEST TD - T7 + 1
		AD	LST1 +6
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	6

# Page 1229
	+4	CCS	A
		AD	LST1 +7
		TCF	+4
		AD	ONE
		TC	WTLST2
		OCT	7

	+4	CCS	A
WTABORT		TC	BAILOUT		# NO ROOM IN THE INN.
		OCT	1203

		AD	ONE
		TC	WTLST2
		OCT	10

OCT40201	OCT	40201

# Page 1230
# THE ENTRY TO WTLST2 JUST PRECEDING OCT N IS FOR T  LE TD LE T   -1.
#                                                  N           N+1
#
# (LE MEANS LESS THAN OR EQUAL TO).  AT ENTRY, C(A) = -(TD - T   + 1)
#                                                             N+1
#
# THE LST1 ENTRY-(T   -T +1) IS TO BE REPLACED BY -(TD - T  + 1), AND
#                  N+1  N                                 N
#
# THE ENTRY-(T   - TD + 1) IS TO BE INSERTED IMMEDIATELY FOLLOWING.
#             N+1

WTLST2		TS	WAITTEMP	#	C(A) = -(TD - T + 1)
		INDEX	Q
		CAF	0
		TS	Q		# INDEX VALUE INTO Q.

		CAF	ONE
		AD	WAITTEMP
		INDEX	Q		# C(A) = -(TD - T ) + 1.
		ADS	LST1 -1		#                N

		CS	WAITTEMP
		INDEX	Q
		TCF	WTLST4

# Page 1231
# ENTERS HERE ON T3 RUPT TO DISPATCH WAITLISTED TASK.

T3RUPT		EXTEND
		ROR	SUPERBNK	# READ CURRENT SUPERBANK VALUE AND
		TS	BANKRUPT	# SAVE WITH E AND F BANK VALUES.
		EXTEND
		QXCH	QRUPT

T3RUPT2		CAF	NEG1/2		# DISPATCH WAITLIST TASK.
		XCH	LST1 +7
		XCH	LST1 +6
		XCH	LST1 +5
		XCH	LST1 +4		# 1. MOVE UP LST1 CONTENTS, ENTERING
		XCH	LST1 +3		#    A VALUE OF 1/2 +1 AT THE BOTTOM
		XCH	LST1 +2		#    FOR T6-T5, CORRESPONDING TO THE
		XCH	LST1 +1		#    INTERVAL 81.91 SEC FOR ENDTASK.
		XCH	LST1
		AD	POSMAX		# 2. SET T3 = 1.0 - T2 - T USING LIST 1.
		ADS	TIME3		#    SO T3 WONT TICK DURING UPDATE.
		TS	RUPTAGN
		CS	ZERO
		TS	RUPTAGN		# SETS RUPTAGN TO +1 ON OVERFLOW.

		EXTEND			# DISPATCH TASK.
		DCS	ENDTASK
		DXCH	LST2 +16D
		DXCH	LST2 +14D
		DXCH	LST2 +12D
		DXCH	LST2 +10D
		DXCH	LST2 +8D
		DXCH	LST2 +6
		DXCH	LST2 +4
		DXCH	LST2 +2
		DXCH	LST2

		XCH	L
		EXTEND
		WRITE 	SUPERBNK	# SET SUPERBANK FROM BBCON OF 2CADR
		XCH	L		# RESTORE TO L FOR DXCH Z.
		DTCB

# Page 1232
# RETURN, AFTER EXECUTION OF T3 OVERFLOW TASK:

		BLOCK	02
		COUNT	02/WAIT

TASKOVER	CCS	RUPTAGN		# IF +1 RETURN TO T3RUPT, IF -0 RESUME.
		CAF	WAITBB
		TS	BBANK
		TCF	T3RUPT2		# DISPATCH NEXT TASK IF IT WAS DUE.

		CA	BANKRUPT
		EXTEND
		WRITE	SUPERBNK	# RESTORE SUPERBANK BEFORE RESUME IS DONE

RESUME		EXTEND
		QXCH	QRUPT
NOQRSM		CA	BANKRUPT
		XCH	BBANK
NOQBRSM		DXCH	ARUPT
		RELINT
		RESUME

# Page 1233
# LONGCALL
#
# PROGRAM DESCRIPTION				      DATE- 17 MARCH 1967
# PROGRAM WRITTEN BY W.H. VANDEVER		     LOG SECTION WAITLIST
# MOD BY- R. MELANSON TO ADD DOCUMENTATION	ASSEMBLY SUNDISK REV. 100
#
# FUNCTIONAL DESCRIPTION-
# LONGCALL IS CALLED WITH THE DELTA TIME ARRIVING IN A,L SCALED AS TIME2,TIME1 WITH THE 2CADR OF THE TASK
# IMMEDIATELY FOLLOWING THE TC LONGCALL.  FOR EXAMPLE, IT MIGHT BE DONE AS FOLLOWS WHERE TIMELOC IS THE NAME OF
# A DP REGISTER CONTAINING A DELTA TIME AND WHERE TASKTODO IS THE NAME OF THE LOCATION AT WHICH LONGCALL IS TO
# START
#
# CALLING SEQUENCE-
#		EXTEND
#		DCA	TIMELOC
#		TC	LONGCALL
#		2CADR	TASKTODO
#
# NORMAL EXIT MODE-
#	1). TC		WAITLIST
#	2). DTCB	(TC L+3 OF CALLING ROUTINE 1ST PASS THRU LONGCYCL)
#	3). DTCB	(TO TASKOVER ON SUBSEQUENT PASSES THRU LONGCYCL)
#
# ALARM OR ABORT EXIT MODE-
#	NONE
#
# OUTPUT-
#	LONGTIME AND LONGTIME+1 = DELTA TIME
#	LONGEXIT AND LONGEXIT+1 = RETURN 2CADR
#	LONGCADR AND LONGCADR+1 = TASK 2CADR
#	A = SINGLE PRECISION TIME FOR WAITLIST
#
# ERASABLE INITIALIZATION-
#	A = MOST SIGNIFICANT PART OF DELTA TIME
#	L = LEAST SIGNIFICANT PART OF DELTA TIME
#	Q = ADDRESS OF 2CADR TASK VALUE
#
# DEBRIS-
#	A,Q,L
#	LONGCADR AND LONGCADR+1
#	LONGEXIT AND LONGEXIT+1
#	LONGTIME AND LONGTIME+1
#
# *** THE FOLLOWING IS TO BE IN FIXED-FIXED AND UNSWITCHED ERRASIBLE ***

		BLOCK	02
		EBANK=	LST1
LONGCALL	DXCH	LONGTIME	# OBTAIN THE DELTA TIME

		EXTEND			# OBTAIN THE 2CADR
# Page 1234
		NDX	Q
		DCA	0
		DXCH	LONGCADR

		EXTEND			# NOW GO TO THE APPROPRIATE SWITCHED BANK
		DCA	LGCL2CDR	# FOR THE REST OF LONGCALL
		DTCB

		EBANK=	LST1
LGCL2CDR	2CADR	LNGCALL2

# *** THE FOLLOWING MAY BE IN A SWITCHED BANK, INCLUDING ITS ERASABLE ***

		BANK	01
		COUNT	01/WAIT

LNGCALL2	LXCH	LONGEXIT +1	# SAVE THE CORRECT BB FOR RETURN
		CA	TWO		# OBTAIN THE RETURN ADDRESS
		ADS	Q
		TS	LONGEXIT

# *** WAITLIST TASK LONGCYCL ***
LONGCYCL	EXTEND			# CAN WE SUCCESFULLY TAKE ABOUT 1.25
		DCS	DPBIT14		# MINUTES OFF OF LONGTIME
		DAS	LONGTIME

		CCS	LONGTIME +1	# THE REASONING BEHIND THIS PART IS
		TCF	MUCHTIME	# INVOLVED, TAKING INTO ACCOUNT THAT THE
					# WORDS MAY NOT BE SIGNED CORRECTED (DP
					# BASIC INSTRUCTIONS
					# DO NOT SIGN CORRECT) AND THAT WE SUBTRAC-
					# TED BIT14 (1 OVER HALF THE POS. VALUE
					# REPRESENTABLE IN SINGLE WORD)
		NOOP			# CAN'T GET HERE **********
		TCF	+1
		CCS	LONGTIME
		TCF	MUCHTIME
DPBIT14		OCT	00000
		OCT	20000

					# LONGCALL
LASTTIME	CA	BIT14		# GET BACK THE CORRECT DELTA TFOR WAITLIST
		ADS	LONGTIME +1
		TC	WAITLIST
		EBANK=	LST1
		2CADR	GETCADR		# THE ENTRY TO OUR LONGCADR

LONGRTRN	CA	TSKOVCDR	# SET IT UP SO THAT ONLY THE FIRST EXIT IS
# Page 1235
		DXCH	LONGEXIT	# TO THE CALLER OF LONGCALL
		DTCB			# THE REST ARE TO TASKOVER

MUCHTIME	CA	BIT14		# WE HAVE OVER OUR ABOUT 1.25 MINUTES
		TC	WAITLIST	# SO SET UP FOR ANOTHER CYCLE THROUGH HERE
		EBANK=	LST1
		2CADR	LONGCYCL


		TCF	LONGRTRN	# NOW EXIT PROPERLY

# *** WAITLIST TASK GETCADR ***
GETCADR		DXCH	LONGCADR	# GET THE LONGCALL THAT WE WISHED TO START
		DTCB			# AND TRANSFER CONTROL TO IT

TSKOVCDR	GENADR	TASKOVER
